Test project CAR PAINTING

Emirates Skills 2019

Submitted by:

Name: Ryan Puckey

Member : Chief Expert

**DESCRIPTION OF PROJECT AND TASKS**

**The Test project uses three car panels and one non-steel panel. One of the car panels is pre painted at the manufacturing factory.**

|  |  |  |
| --- | --- | --- |
| **Team Leader Module description** | | |
| **Module A** | **Blend pre painted left wing** | **2.0 hrs** |
| **Module B** | **Masking of car and repair pre painted plastic part** | **2.0 hrs** |
| **Module C** | **Standard application inside and outside right door** | **4.0 hrs** |
| **Module D** | **Colour matching** | **2.0 hrs** |
|  |  | **10.0 hrs** |

|  |  |  |
| --- | --- | --- |
| **Colour description…. All colours quantities are RFU!** | | |
| **Colour - 2Stage**  **Colour - 2Stage** | **Inside right door**  **Outside right door** | **Code: TOY – 5B5**  **350 Gram**  **Code: Merc Benz - 744**  **350 Gram** |
| **Colour - No paint** | **Non steel panel** | **Code: TOY 1E3** |
| **Colour- 2Stage** | **Spot repair left wing-Pre painted** | **Code: TOY 8R3**  **Hole Panel: 400 Gram**  **Repair: 100 Gram** |


**A number of colour codes will be decided by the judging panel at the competition**

|  |  |
| --- | --- |
| **Panels description** | |
| **Panel # 1** | **Pre painted left wing** |
| **Panel # 2** | **Pre painted front bumper** |
| **Panel # 3** | **OEM replacement front door** |

**There will be an introduction 5-10 minutes before each module**

**Please Take Note of these Symbols**

** You must stop and have your work judged**

** Turn in sprayout sample**

**Instruction to the Competitor**

|  |  |
| --- | --- |
| **Module A: 2-layer - Blend pre-painted panel –using pre mixed paint.**    **Apply colour. Colour on the fender is an off colour from a colour swatch variant. You will be supplied with premixed paint** | **Time allowed 2.0 HRS** |
| **Prep panel for blending - (Panel # 3)**   * **Repair scratch** * **Apply Primer Filler** * **Prep for base** | **MCj04298170000[1]**  **MCj04298170000[1]** |
| **Apply basecoat and clear coat**   * **You must limit the extent of the clear coat to the boundary indicated in the drawing CP3** |  |
| * **Once the spot repair has been marked/scored you can polish the repair**   **Note : The panels must be painted and dried in a vertical position** | **MCj04298170000[1]** |

|  |  |
| --- | --- |
| **Module B: Masking /Featheredge, prime and block.**  **The time allotted for both task.**  **(Panel#5 for plastic repair)** | **Time allowed 2.0 HRS** |
| * **Masking side of vehicle/car/and jambs** |  |
| * **Expert will evaluate masking outline** |  |
| **Plastic part** |  |
| * **Repair scratch in paint** |  |
| * **Apply body filler** |  |
| * **Prep for paint** |  |

|  |  |
| --- | --- |
| **Module C: Standard application, inside and outside door** | **Time allowed 4.0 HRS** |
| * **Use the OEM replacement door (Panel # 2)** |  |
| * **Check Door for prior damage and notify expert if you see any.** * **Prepare damaged area for polyester filler** * **Apply polyester filler to damaged area and sand** * **Prepare entire door for primer application** * **outside must be in primer surfacer** * **inside can be primer surfacer or wet-on-wet** * **Apply primer surfacer on inside and outside of door if chosen** * **Prepare for base and apply wet –on-wet if chosen** * **Apply base and clear**   **Note : The panels must be painted in a vertical position** |  |

|  |  |
| --- | --- |
| **Module D: Colour mixing** | **Time allowed 2.0 HRS** |
| * **Using supplied colour sample- mix from scratch #1** |  |
| * **Make colour to match the given sample** |  |
|  |  |
| * **After completing colour adjustment turn in the sample colours applied to spray out card that you would like to have evaluated** | **MCj04356040000[1]** |
|  |  |
| **Note: You cannot use the scales or computers for this process** |  |